# Annex No. 6  Technical Specification of the Supply

# Technical parameters table

|  |  |  |
| --- | --- | --- |
| **Parameter** | **Required value** | **Offered value** |
| Mode of operation | Fully automated |  |
| INP concentration range | 0.002 – 1000 L-1 |  |
| Particle detection range | 0.2 – 200 µm |  |
| Possibility to do ice nucleation and INP measurements | -10°C to -65°C |  |
| Dimensions | height 2 m max, width 1 m max, depth 1 m max |  |
| Power consumption | 1 kW max |  |
| Working temperature | 15 ºC - 35ºC |  |
| Weight | 250 kg max |  |